CONGRATULATIONS
Dear Owner,
Thank you for buying a SOVEMA manufactured product.
Your new machine is carefully designed and manufactured to give you superior performance and dependable service, if properly operated and maintained.
You will find this machine to be rugged and reliable when matched to the suggested horsepower operating range.
Much time has been invested in providing safety and protection. Please carefully read this manual. It tells you how to safely and easily assemble, operate and maintain your machine.
Be sure that you and any other operator carefully follow the recommended safety practices at all times. Failure to do so could result in personal injury or property damage.
Of course, if you should ever have any problems or questions, please contact your local SOVEMA dealer or contact us at the addresses or numbers indicated in this manual.
SOVEMA manufactures a variety of innovative equipment. If you are interested in reviewing our full line, please contact us.
Thanks for your choice.
Silvio Mayer
President

Pag.#

TABLE OF CONTENTS
- SYMBOLS Page 3
- GENERAL INFORMATION Page 4
- SAFETY AND WARNING DECALS Page 5
- SAFETY INSTRUCTIONS Page 7
- MAIN CHECK Page 10
- TECHNICAL SPECIFICATIONS Page 11
- ATTACHING THE MACHINE TO THE TRACTOR Page 14
- DEPTH CONTROL Page 18
- BEGINNING WORK Page 21
- TROUBLE SHOOTING Page 22
- DISCONNECTING THE MACHINE FROM THE TRACTOR Page 24
- STORING OF THE MACHINE Page 25
- MAINTENANCE Page 26
- TOXICOLOGICAL INFORMATION Page 29
- SPARE PARTS LIST Page 31
- WARRANTY POLICY Page 42
- SOVEMA PRODUCT LINE

Pag.#

SYMBOLS
These symbols appear throughout the manual.
Remember their meaning and advice.

MEANS: CAUTION!
YOUR SAFETY IS INVOLVED

MEANS: READ CAREFULLY

MEANS: USE PROTECTIVE GLOVES

Pag.#

GENERAL INFORMATION
All implements with moving parts are potentially hazardous. The manufacturer has designed the implement to be used with all the safety equipment properly attached. The purpose of this manual is to assist you in safety maintaining and operating the implement.
These instructions have been compiled from our experience.
Through this experience and these instructions, you should be able to develop operating procedures suitable to your particular situation.
Illustrations and data used in this manual may vary slightly in some details. Throughout this manual references are made in left and right directions. These are determined by standing at the rear of the equipment and facing the direction of forward travel.
Even if some illustrations in this manual show the machine with safety shields removed for a better view, never operate in these conditions.
BEFORE OPERATING THE IMPLEMENT, ALL SAFETY SHIELDS OR DEVICES MUST BE MOUNTED

RIGHT

LEFT

Pag.#

SAFETY AND WARNING DECALS
Safety decals on the implement contain important safety warning messages. To prevent injuries we invite the operator to read them carefully and keep them clear. Check that all the decals are on the machine. If not, DO NOT USE the machine and report to the Dealer immediately to get the decals. Decals on the machine are the following and mean:
1 2 3 4
1. Before operating the equipment, read carefully the operator’s manual.
2. Before maintenance operation, lower the implement, shut off the engine and read the operator’s manual.
3. Do not allow riders on tractor or implement.
4. Do not stand behind the tractor during the operations.
5. Before operating the equipment, read carefully the operator's manual.
6. DANGER! Entanglement of driveline..
7. KEEP AWAY from driveline in operation: contact can cause death!

Pag.#

8. Danger. Your hands and feet can be injured by moving parts. Keep away from the implement.
9. Danger. Your hands can be injured. Do not remove the cover and keep away from moving parts.
10. Danger. Your hands can be injured. Do not remove safety protection and keep away from moving parts.
11. Danger. Your hands can be injured. Do not remove the cover and keep away from moving parts.
12. The machine is designed for use on tractors with 540 RPM PTO only
13. Caution! During working operations all bystanders must stay beyond the shown distances from the implement.

8

9

10

11

Pag.#

SAFETY INSTRUCTIONS
Before using the implement you must be sure to know the main safety precautions; in fact many accidents are caused by not observing these rules.
Pre-operational and operational safety rules
Make sure that no person operates this machine unless they first, thoroughly read and studied the operator instructions for this machine and understood all the safety precautions.
Keep all guards, shields and safety decals in place and proper working order before operating this machine.
Operate only with a tractor equipped with an approved Roll Over Protective System (ROPS) and always wear your seat-belt.
Operate only in daylight or good artificial light.
Only trained personnel can operate with the tractor and the implement.
Personal protection equipment, including safety shoes, safety glasses, hard hat and gloves are recommended during the different operations. Do not allow long hair, loose fitting clothing or jewellery to be around moving parts.
Do not leave the tractor seat until the engine is completely turned off, brakes locked and ignition key removed.
Do not allow riders on the machine or tractor at any time. No safe place for any rider.
Before starting to operate, be sure that the tractor's PTO is set to match the PTO requirements of the implement. The speed is indicated in this manual and on the implement.
Do not use different driveline . Always use type and size supplied by the manufacturer.
Make sure driveline spring-activated locking pin operate freely and are seated firmly in tractor PTO stub shaft groove.

Pag.#

For engaging or disengaging the tractor PTO, refer to your tractor manual.
Connect and disconnect PTO shaft only when tractor engine is turned off.
Keep hands, feet, hair and clothing away from moving parts.
To prevent injury by thrown objects DO NOT operate unless all personnel, livestock and pets are 20 m (65 ft) away.
The rotating parts of the machine have been designed and tested for rugged use. However they could fail upon impact with heavy solid objects. Such impact could cause the broken objects to be thrown outward at very high speed. To reduce the possibility of serious injury, or even death, never allow the rotating parts to contact such obstacles.
Stop the machine and tractor immediately upon striking an obstruction. Turn engine off, remove key, inspect and repair any damage before resuming operation.
No repairs or adjustments should be attempted while the machine is attached to a tractor that is turned on.
Working inclination of PTO driveline must not exceed 25° (see fig.1). Greater working angles will damage the PTO and serious personal injury could occur as well.
Disengage tractor PTO and place transmission into neutral before attempting to start engine.
Transport safety
Plan your route to avoid heavy traffic.
For public roads, comply with state and local safety and movement rules.
Be sure that the implement is in the raised position for transport.

Pag.#

When you must drive, do not drink.
Pay attention to traffic when operating near or crossing roadways.
Reduce speed when transporting mounted implement to avoid bouncing and loss of steering control.
Pay attention when you turn curves or you go up and down on hills with the implement. Be sure that at least 25% of the tractor’s weight is on the front wheels to maintain safe steering. Drive at a low speed.
NEVER allow riders on implement or tractor. Falling off can kill.
Be a safe and courteous driver.
Maintenance safety
Good maintenance is your responsibility. Poor maintenance is an invitation to trouble.
For maintenance follow these common practises:
- keep service area clean;
- use adequate illumination for the job;
- be sure tools and electrical outlets are properly grounded;
- make sure there is plenty of ventilation.
Before making maintenance on this machine, drive to a level area, disengage the PTO, lower the machine, turn off the engine, set the brakes and remove the ignition key.
Keep all persons away from operator control area while performing maintenance.
ALWAYS use personal protection devices.
Periodically tighten all bolts, nuts and screws.
The implement manufacturers assumes no liability if replacement parts other than the original factory parts are used.
After servicing, be sure that all safety shields are re-installed properly.
Be sure that all safety decals are installed, clean and in good condition.
If the machine is modified from the original design, no responsibility for the manufacturer
can be claimed.

Pag.#

MAIN CHECK LIST
Before connecting the machine to the tractor, read the following instructions:
Be sure the weight and power of the tractor is correct with the machine you want to connect. If you have any doubt, see the technical specifications.
Ensure that all safety decals are properly installed and clean.
Check oil in the gearbox and into side transmission cover. With low oil, gears get damaged.
Be sure that all safety shielding is properly installed and in good condition.

Pag.#

TECHNICAL SPECIFICATIONS
The machine described in this manual is a rotary tiller of the GDT series.

Pag.#

LEVEL OF NOISE RESULT WHEN IDLING

83

Pag.#

SPEED CHART FOR GDT

Pag.#

ATTACHING THE MACHINE TO THE TRACTOR
The machines described in this manual do apply to any kind of tractor provided of universal third hitch point.
The characteristics (length, diameter of the holes for the lifting pins) of the tractor’s lifting arms depend on the type of tractor, therefore it is necessary to prepare the machine in order to conclude the attachment correctly.
Before attaching the machine to the tractor you must be sure that the engine is turned off, brakes are locked and the ignition key is removed.
This operation must be made on a flat area as it is very dangerous.
Do not allow anyone between tractor and implement when the engine is running.
Follow these instructions:
Connect the hitch of the drawbar to the tractor using a hitch pin and the hair clip pin (see fig. 1)

LOWER PLATES

FIG. 1

Pag.#

Connect the third point of the tractor to the upper plates of the machine using a hitch pin and the hair clip pin (see fig. 2). By means of the tie rod of the hitch point, which permits regulation of the machine's inclination, set the machine even to ground-floor (see fig. '3). This procedure extends life time of the PTO shaft and the machine.
Connect the PTO shaft and be sure it is correctly connected to the tractor and the machine (see fig.4).

UPPER
PLATES

FIG. 3

FIG. 2

FIG. 4

Pag.#

Shortening the PTO shaft
Due to the many different types of tractors, it may be necessary to shorten the PTO shaft.
Always refer to the manual of the driveline’s manufactures. Read it carefully.
In case shortening is needed, listed below are some basic guidelines on performing this modification. Determine how much length is to be removed, then:
Remove plastic protection (both sections)
2) Cut the excess length of both tubes
3) Deburr and clean the saw-dust off ends of tubes. Remove packing inside shaft tubing

1

2

3

Pag.#

4) Cut the plastic protection to the same length you have cut the joints
5) Grease the male joint section and reassemble protection
Do not use PTO shafts without proper shielding installed.

4

5

Pag.#

DEPTH CONTROL
To set the machine's working depth, adjust the two lateral skids as in figure 1:
Loosen screw "a".
Unscrew screw "b".
Adjust the skid as wished screwing down screw "b" in one of the holes located in the same skid.
Tighten screws “a” and “b”.
To get on even soil, make sure that both skids are at the same position.
If your machine is equipped with a rear roller, depth adjustment is carried out by a crank (fig. 2).

a

skid

FIG. 1

b

Pag.#

GEAR SPEED— GDT Series
These machines are equipped with a 4 speed gearbox, which permits to change the rotor speed.
Higher rotor speed allows better tilling of the soil.
To change speed you must follow next steps:
Pay attention: oil can come aut, so position the machine in a way that rear part is higher than front part.
Unscrew its bolts and remove the rear cover of the gearbox.
According to the required speed, change position of the gears (See chart in chapter on Technical Specifications).
Mount again the rear cover and screw the bolts.
Be very careful and ensure to use the right gears, since some gear pairs cannot be inverted, and gears from different pairs cannot be interchanged. Use only original gears!

crank

FIG. 2

Pag.#

Be very careful and ensure to use the right gears, since some gear pairs cannot be inverted, and gears from different pairs cannot be interchanged. Use only original gears!

Pag.#

BEGINNING WORK
After completing all safety controls, to avoid damage start as follows:
Raise the machine off the ground in order to let the blades start moving without touching ground.
Maintaining the machine raised, engage the tractor PTO at suggested engine RPM.
Start moving the tractor forward and then gradually lower the machine.
TIPS TO GET DESIRED RESULTS
Proper ground speed of the machine depends on the type of terrain to work. However it is advisable not to exceed 5 Km/h.
For a very fine seedbed, lower the rear shield completely and operate at a very slow speed. For a more coarse seedbed, raise the shield and/or increase operating speed, not exceeding the speed suggested before.
While operating, to avoid damage do not attempt to make turns and do not absolutely go backwards. Disengage the machine and raise it off the ground when making turns and U turns.

Pag.#

Pag.#

TROUBLE SHOOTING
During work several problems can happen:
Unusual noise
While working, if the machine made unusual noise, the operator must stop it immediately and follow next instructions:
Check for broken/bent parts.
• Check for a sudden movement of the lateral cover after a casual impact.
In fact, a sudden impact with an obstacle can move the cover out of place causing oil leaking. This can make the gears not be correctly lubricated and become noisy, and with time brake apart.
• Check for correct oil level in the gearbox.
When present incorrect oil level (see chapter on maintenance), the gears of the gearbox are not lubricated correctly, and if continue to rotate, would determine a significant increase in oil temperature. If continue working in this condition will quickly take to damage gear bearings.
• Check condition of rotor support bearings.
Inadequate lubrication (see chapter on maintenance) may cause damage on one of the two rotor support bearings. The rotor begins to oscillate causing excessive vibration to the frame and in short time, the damage of its weldings.
Another possible cause for bearing damage is the improper use of the machine: high ground speed, turns/U turns, going backwards, or operating in soil with high rock content.

Pag.#

Pag.#

Problem with uniformity on result
While operating, if you notice that work is not uniform, stop the machine and check that no object has been trapped in the rotor.
Before checking the machine to find the possible cause of the problem, be sure the tractor's PTO is disconnected, tractor's engine turned off, brakes on, key ignition off the command board, and the machine completely lowered to the ground.

Pag.#

Pag.#

DISCONNECTING THE MACHINE FROM THE TRACTOR
Disconnecting of the machine must be carried out on flat area, and it is considered a very dangerous operation. You must pay attention. Follow these instructions:
While remaining in the tractor seat, put the tractor PTO in neutral.
When the rotors are completely stopped, turn off the engine and set the parking brakes.
Remove the ignition key.
Descend from the tractor and disconnect the driveline.
If you have an hydraulic fold machine, disconnect hydraulic hoses from the tractor.
Engage the parking stand.
Disconnect the hitch of the drawbar from the tractor.
Before disconnecting the driveline, be sure the tractor PTO is in neutral and engine is off.

Pag.#

STORING OF THE MACHINE
As your machine is an investment and if remains unused for a long period, we suggest the following procedures:
Wash and dry the machine;
Check all moving parts. For excessive wear replace the parts or contact your local dealer;
Check bolts and nuts for proper tightness;
Lubricate all the active parts like bearings, all grease zerk locations and other pivot or worn points that may not have a fitting.
Lubricate all not-painted parts;
Store the machine in a clean and dry place under roof.

Pag.#

MAINTENANCE
For long life of your machine and trouble free operation, regular program of maintenance is required.
The recommended phases of maintenance are for normal use and can be varied depending on the different conditions.
Always disengage tractor PTO before starting maintenance.
Every 10 working hours
Check far loose bolts that fix the blades to the rotor. Tighten as needed (see fig. 1).
Grease the PTO shaft components.
Clean the end of PTO shaft with non toxic / non inflammable detergent.
Be sure that driveline shields are in place and in good condition.
Grease the right lateral support of the rotor (see fig. 2) after cleaning correctly the grease nipples for better lubrication. Use lithium type grease NLGI 2 .
Clean the machine.

Pag.#

Every 50 working hours
Check blades for wear. Replace if necessary. Use only original parts.
Make sure PTO shaft and slip clutch are in place and in good condition. If damaged or worn, replace slip discs. Contac your local dealer for substitution.
For those machines supplied with rear roller, grease the screw and lateral supports, after cleaning correctly the grease nipples for better lubrication, Use lithium type grease NLGI 2.
Check oil level in the gearbox.
For versions (GDE and GDEC), this operation is carried out by unscrewing the plug located on top of the box (1 in fig. 3) and checking the oil measurer supplied with the plug. Maximum oil level is 3 cm above the bottom of the measurer.

Grease nipple

FIG. 1

FIG. 2

1

Small rod

2

FIG. 3

FIG. 3

Pag.#

Check oil level in the cover gear by unscrewing the oil level plug (2 in fig. 4). If needed to add oil, unscrew the filler plug (3 in fig. 4) and fill in the cover until oil starts running out of the level hole.
First 100 working hours
In the case the machine has done its first 100 hours, change oil in the gearbox and gear drive.
To change oil In the gearbox, unscrew the plug located on top of the box inclining opportunely the machine.
To change oil in the cover, drain all the oil from the level hole located on the lower part of it (always after inclining the machine).
These changes are necessary because the gears are new and so are subject to quicker worn. Use oil: SAE 80 W 90 API GL 4.
Every 300 working hours
Completely replace oil in the gearbox and gear drive, as explained before, Use oil: SAE 80 W 90 API GL 4 .

3

2

FIG. 4

Pag.#

TOXICOLOGICAL INFORMATION ABOUT LUBRICANTS

	TYPES OF DANGER	PROTECTIVE EQUIPMENT	PRIMARY INTERVENTION
SKIN	Possible irritation after prolonged contact	Gloves and/or lotion barrier	Wash with soap & water
EYES	Possible irritation on contact	Protective goggles	Rinse thoroughly w/ running water
INHALATION	Possible irritation after prolonged exposure	Maintain an oil mist level of 5mg/m3 between TLV-TWA limits	Expose to fresh air and call medical assistance immediately
INGESTION	Such possibility not considered		DO NOT provoke vomiting; call medical assistance immediately

Pag.#

USE EXLUSIVELY ORIGINAL SPARE PARTS FROM
SOVEMA

Pag.#

SPARE PARTS LIST
GDT Model

Pag.#

GDT
Frame

Pag.#

REF	CODE	QTY	ENGLISH	FRANÇAIS	ITALIANO	DEUTSCH	ESPAÑOL	NOTE
1	900.142.236	1	FRAME	CHASSIS	TELAIO	RAHMEN	BASTIDOR	230
1	900.142.237	1	FRAME	CHASSIS	TELAIO	RAHMEN	BASTIDOR	250
1	900.142.238	1	FRAME	CHASSIS	TELAIO	RAHMEN	BASTIDOR	280
1	900.142.239	1	FRAME	CHASSIS	TELAIO	RAHMEN	BASTIDOR	300
2	900.142.231	1	SIDE	FLANC	FIANCO	SEITE	FLANCO
3	900.142.230	1	PLATE	PLAQUE	PIASTRA	PLATTE	PLACA
4	900.115.032	1	SKID	PATIN	SLITTA	KUFE	CORREDERA
5	900.115.011	2	ROD	TIGE	ASTA	STANGE	VARILLA
6	900.115.033	1	SKID	PATIN	SLITTA	KUFE	CORREDERA
7	900.142.240	1	SUPPORT	SUPPORT	SUPPORTO	STUETZE	SOPORTE
8	900.238.001	1	STAND	SUPPORT	SOSTEGNO	STUETZE	SOPORTE
9	900.108.005	1	SPLIT PIN R 3	GOUPILLE R 3	COPIGLIA R 3	ARRETIERUNG R 3	PASADOR R 3
10	900.207.008	1	PIN	CHEVILLE	SPINA	DORN	CLAVIJA
11	900.116.119	2	FLASK	MOULE	STAFFA	KLAUE	PLETINA
12	900.116.117	2	HITCH	ATTELAGE	ATTACCO	ANBAU	ENGANCHE
13	900.102.154	4	SCREW M 18x50	VIS M 18x50	VITE M 18x50	SCHRAUBE M 18x50	TORNILLO M 18x50
14	900.104.113	4	WASHER GROWER 18 R	RONDELLE GROWER 18 R	RONDELLA GROWER 18 R	ZWISCHENSC. GROWER 18 R	ARANDELA GROWER 18 R
15	900.103.017	4	NUT M 18	ECROU M 18	DADO M 18	MUTTER M 18	TUERCA M 18
16	900.102.102	2	SCREW M 12x35	VIS M 12x35	VITE M 12x35	SCHRAUBE M 12x35	TORNILLO M 12x35
17	900.104.046	14	WASHER 12x24	RONDELLE 12x24	RONDELLA 12x24	ZWISCHENSCHEIBE 12x24	ARANDELA 12x24
18	900.103.019	14	NUT BLOK M12	ECROU BLOK M12	DADO BLOK M12	MUTTER BLOK M12	TUERCA BLOK M12
19	900.102.031	2	SCREW M14x60	VIS M 14x60	VITE M 14x60	SCHRAUBE M 14x60	TORNILLO M 14x60
20	900.102.027	14	SCREW M 14x35	VIS M 14x35	VITE M 14x35	SCHRAUBE M 14x35	TORNILLO M 14x35
21	900.103.005	24	NUT M 14	ECROU M 14	DADO M 14	MUTTER M 14	TUERCA M 14
22	900.104.061	18	WASHER GROWER 14 R	RONDELLE GROWER 14 R	RONDELLA GROWER 14 R	ZWISCHENSC. GROWER 14 R	ARANDELA GROWER 14 R
23	900.142.232	1	LAND COVER	TOLE PARE-TERRE	LAMIERA PARATERRA	BLECH BODEN-SCHUTZT	CHAPA PARA-TIERRA
24	900.142.233	1	LAND COVER	TOLE PARE-TERRE	LAMIERA PARATERRA	BLECH BODEN-SCHUTZT	CHAPA PARA-TIERRA
25	900.102.028	6	SCREW M 14x40	VIS M 14x40	VITE M 14x40	SCHRAUBE M 14x40	TORNILLO M 14x40
26	900.139.114	1	GASKET	JOINT	GUARNIZIONE	DICHTUNG	JUNTA
27	900.113.024.0	1	COVER	CARTER	CARTER	GEHAUSE	CARTER
28	900.102.050	1	PLUG	BOUCHON	TAPPO	DECKEL	TAPON
29	900.102.008	18	SCREW M 8x25	VIS M 8x25	VITE M 8x25	SCHRAUBE M 8x25	TORNILLO M 8x25
30	900.104.002	18	WASHER DENT. 8	RONDELLE DENT. 8	RONDELLA DENT. 8	ZWISCHENSCHEIBE DENT. 8	ARANDELA DENT. 8
31	900.103.001	18	NUT M 8	ECROU M 8	DADO M 8	MUTTER M 8	TUERCA M 8
32	900.104.009	1	WASHER 10x16x1.5 AL	RONDELLE 10x16x1.5 AL	RONDELLA 10x16x1.5 AL	ZWISCHENSC. 10x16x1.5 AL	ARANDELA 10x16x1.5 AL
33	900.102.009	1	SCREW M 10x10	VIS M 10x10	VITE M 10x10	SCHRAUBE M 10x10	TORNILLO M 10x10
34	900.114.133	1	SHIELD R	CAPOT D	COFANO DX	HAUBE R	CARCASA D	230
34	900.114.135	1	SHIELD R	CAPOT D	COFANO DX	HAUBE R	CARCASA D	250
34	900.114.137	1	SHIELD R	CAPOT D	COFANO DX	HAUBE R	CARCASA D	280
34	900.114.139	1	SHIELD R	CAPOT D	COFANO DX	HAUBE R	CARCASA D	300
35	900.114.134	1	SHIELD L	CAPOT G	COFANO SX	HAUBE L	CARCASA I	230
35	900.114.136	1	SHIELD L	CAPOT G	COFANO SX	HAUBE L	CARCASA I	250
35	900.114.138	1	SHIELD L	CAPOT G	COFANO SX	HAUBE L	CARCASA I	280
35	900.114.140	1	SHIELD L	CAPOT G	COFANO SX	HAUBE L	CARCASA I	300
36	900.211.028	2	BUSH	COQUILLE	BOCCOLA	BUCHSE	CASQUILLO
37	900.104.043	26	WASHER 17x30x3	RONDELLE 17x30x3	RONDELLA 17x30x3	ZWISCHENSCHEIBE 17x30x3	ARANDELA 17x30x3
38	900.103.023	18	NUT BLOK M16	ECROU BLOK M 16	DADO BLOK M16	MUTTER BLOK M16	TUERCA BLOK M16
39	900.116.106	2	FLASK	MOULE	STAFFA	KLAUE	PLETINA
40	900.116.118	2	FLASK	MOULE	STAFFA	KLAUE	PLETINA
41	900.102.096	16	SCREW M 14x40	VIS M 14x40	VITE M 14x40	SCHRAUBE M 14x40	TORNILLO M 14x40
42	900.104.044	44	WASHER 15x28x2.5	RONDELLE 15x28x2.5	RONDELLA 15x28x2.5	ZWISCHENSC. 15x28x2.5	ARANDELA 15x28x2.5
43	900.103.021	36	NUT BLOK M 14	ECROU BLOK M14	DADO BLOK M14	MUTTER BLOK M14	TUERCA BLOK M14
44	900.102.112	12	SCREW M 14x45	VIS M 14x45	VITE M 14x45	SCHRAUBE M 14x45	TORNILLO M 14x45
45	900.102.235	8	SCREW M 16x50	VIS M 16x50	VITE M 16x50	SCHRAUBE M 16x50	TORNILLO M 16x50
46	900.102.255	8	SCREW M 14x65	VIS M 14x65	VITE M 14x65	SCHRAUBE M 14x65	TORNILLO M 14x65
47	900.114.044	4	PIN	TOURILLON	PERNO	STIFT	PERNO
48	900.108.006	1	SPLIT PIN R 4	GOUPILLE R 4	COPIGLIA R 4	ARRETIERUNG R 4	PASADOR R 4
49	900.114.130	8	ROD	TIGE	ASTA	STANGE	VARILLA
50	900.114.131	4	ROD	TIGE	ASTA	STANGE	VARILLA
51	900.114.132	8	SHIELD SPRING	RESSORT CAPOT	MOLLA COFANO	FEDER HAUBE	MUELLE CARCASA
52	900.116.115	4	U-BOLT	MANILLE	CAVALLOTTO	U-BOLZEN	SOPORTE
53	900.117.103	4	FLASK	MOULE	STAFFA	KLAUE	PLETINA
54	900.117.109	6	GUARD	PROTECTION	PROTEZIONE	SCHUTZ	PROTECCION	230
54	900.117.110	6	GUARD	PROTECTION	PROTEZIONE	SCHUTZ	PROTECCION	250
54	900.117.111	6	GUARD	PROTECTION	PROTEZIONE	SCHUTZ	PROTECCION	280
54	900.117.112	6	GUARD	PROTECTION	PROTEZIONE	SCHUTZ	PROTECCION	300
55	900.117.104	4	FLASK	MOULE	STAFFA	KLAUE	PLETINA
56	900.102.171	8	SCREW M 10x55	VIS M 10x55	VITE M 10x55	SCHRAUBE M 10x55	TORNILLO M 10x55
57	900.104.045	12	WASHER 10.5x21x2	RONDELLE 10.5x21x2	RONDELLA 10.5x21x2	ZWISCHENSC. 10.5x21x2	ARANDELA 10.5x21x2
58	900.103.018	16	NUT BLOK M 10	ECROU BLOK M 10	DADO BLOK M 10	MUTTER BLOK M 10	TUERCA BLOK M 10
59	900.117.102.1	4	SUPPORT	SUPPORT	SUPPORTO	STUETZE	SOPORTE
60	900.102.100	4	SCREW M 10x30	VIS M 10x30	VITE M 10x30	SCHRAUBE M 10x30	TORNILLO M 10x30
61	900.102.169	4	SCREW M 10x40	VIS M 10x40	VITE M 10x40	SCHRAUBE M 10x40	TORNILLO M 10x40
62	900.117.107	2	GUARD	PROTECTION	PROTEZIONE	SCHUTZ	PROTECCION
63	900.116.124	1	HITCH	ATTELAGE	ATTACCO	ANBAU	ENGANCHE
64	900.116.125	1	SIDE R	FLANC D	FIANCO DX	SEITE R	FLANCO D
65	900.116.126	1	SIDE L	FLANC G	FIANCO SX	SEITE L	FLANCO I
66	900.102.095	8	SCREW M 16x40	VIS M 16x40	VITE M 16x40	SCHRAUBE M 16x40	TORNILLO M 16x40
67	900.102.102	4	SCREW M 12x35	VIS M 12x35	VITE M 12x35	SCHRAUBE M 12x35	TORNILLO M 12x35

Pag.#

GDT
Gearbox

Pag.#

REF	CODE	QTY	ENGLISH	FRANÇAIS	ITALIANO	DEUTSCH	ESPAÑOL	NOTE
1	900.148.012	1	CASE	BOITE	SCATOLA	KISTE	CAJA
2	900.148.013	1	GEAR	ENGRENAGE	INGRANAGGIO	ZAHNRAD	ENGRANAJE
3	900.148.014	1	GEAR	ENGRENAGE	INGRANAGGIO	ZAHNRAD	ENGRANAJE
4	900.139.112	2	GASKET	JOINT	GUARNIZIONE	DICHTUNG	JUNTA
5	900.107.010	1	SHIM	EPAISSEUR REG.	SPESSORE REG.	STAERKE	ESPESOR REG.
6	900.102.011	22	SCREW M 10X25	VIS M 10x25	VITE M 10x25	SCHRAUBE M 10x25	TORNILLO M 10x25
7	900.148.015	1	CROWN	COURONNE	CORONA	TELLERRAD	CORONA
8	900.119.082	1	TUBE	TUBE	CANNOTTO	ROHR	TUBO	230
8	900.119.060	1	TUBE	TUBE	CANNOTTO	ROHR	TUBO	250
8	900.119.042	1	TUBE	TUBE	CANNOTTO	ROHR	TUBO	280
8	900.119.061	1	TUBE	TUBE	CANNOTTO	ROHR	TUBO	300
9	900.100.021	1	BEARING 30214	ROULEMENT 30214	CUSCINETTO 30214	KUGELLAGER 30214	COJINETE 30214
10	900.103.062	1	RING NUT BLOK M45x1.5	EMBOUT BLOK M45x1.5	GHIERA BLOK M45x1.5	NUTMUTTER BLOK M45x1.5	CASQUILLO M45x1.5
11	900.148.016	1	PINION	PIGNON	PIGNONE	RITZEL	PINON
12	900.100.109	1	BEARING 6411	ROULEMENT 6411	CUSCINETTO 6411	KUGELLAGER 6411	COJINETE 6411
13	900.101.034	1	OIL SEAL 55x85x10	PARE-HUILE 55x85x10	PARAOLIO 55x85x10	SIMMERRING 55x85x10	PARA-ACEITE 55x85x10
14	900.118.087	1	SHAFT	ARBRE	ALBERO	WELLE	EJE	230
14	900.118.055	1	SHAFT	ARBRE	ALBERO	WELLE	EJE	250
14	900.118.068	1	SHAFT	ARBRE	ALBERO	WELLE	EJE	280
14	900.118.056	1	SHAFT	ARBRE	ALBERO	WELLE	EJE	300
15	900.101.068	1	OIL SEAL 65x85x10	PARE-HUILE 65x85x10	PARAOLIO 65x85x10	SIMMERRING 65x85x10	PARA-ACEITE 65x85x10
16	900.105.021	1	GREASE NIPPLE M10x1	GRAISSEUR M10x1	INGRASSATORE M10x1	SCHMIERNIPPEL M10x1	ENGRASADOR M10x1
17	900.100.110	1	BEARING 32211	ROULEMENT 32211	CUSCINETTO 32211	KUGELLAGER 32211	COJINETE 32211
18	900.102.239	2	SCREW M8x40	VIS M 8x40	VITE M 8x40	SCHRAUBE M 8x40	TORNILLO M 8x40
19	900.148.017	1	SHAFT	ARBRE	ALBERO	WELLE	EJE
20	900.148.018	1	LID	COUVERCLE	COPERCHIO	DECKEL	TAPA
21	900.102.079	1	PLUG	BOUCHON	TAPPO	DECKEL	TAPON
22	900.102.157	1	PLUG	BOUCHON	TAPPO	DECKEL	TAPON
23	900.148.003	1	BUSH	COQUILLE	BOCCOLA	BUCHSE	CASQUILLO
24	900.148.019	1	SHAFT	ARBRE	ALBERO	WELLE	EJE
25	900.107.054	2	SHIM	EPAISSEUR REG.	SPESSORE REG.	STAERKE	ESPESOR REG.
26	900.102.012	4	SCREW M10x30	VIS M10x30	VITE M 10x30	SCHRAUBE M 10x30	TORNILLO M 10x30
27	900.148.020	1	LID	COUVERCLE	COPERCHIO	DECKEL	TAPA
29	900.107.065	1	SHIM	EPAISSEUR REG.	SPESSORE REG.	STAERKE	ESPESOR REG.
30	900.101.023	1	OIL SEAL 45x80x10	PARE-HUILE 45x80x10	PARAOLIO 45x80x10	SIMMERRING 45x80x10	PARA-ACEITE 45x80x10
31	900.100.024	1	BEARING 30309	ROULEMENT 30309	CUSCINETTO 30309	KUGELLAGER 30309	COJINETE 30309
32	900.123.082	1	DOUBLE TUBE	DOUBLE TUBE	DOPPIO CANNOTTO	DOPPELROHR	DOBLE TUBO	230
32	900.123.083	1	DOUBLE TUBE	DOUBLE TUBE	DOPPIO CANNOTTO	DOPPELROHR	DOBLE TUBO	250
32	900.123.084	1	DOUBLE TUBE	DOUBLE TUBE	DOPPIO CANNOTTO	DOPPELROHR	DOBLE TUBO	280
32	900.123.085	1	DOUBLE TUBE	DOUBLE TUBE	DOPPIO CANNOTTO	DOPPELROHR	DOBLE TUBO	300
33	900.107.041	2	SHIM	EPAISSEUR REG.	SPESSORE REG.	STAERKE 32209	ESPESOR REG.
34	900.100.111	2	BEARING 32209	ROULEMENT 32209	CUSCINETTO 32209	KUGELLAGER	COJINETE 32209
35	900.148.021	1	GEAR	ENGRENAGE	INGRANAGGIO	ZAHNRAD	ENGRANAJE
36	900.148.022	1	GEAR	ENGRENAGE	INGRANAGGIO	ZAHNRAD	ENGRANAJE
37	900.139.113	1	GASKET	JOINT	GUARNIZIONE	DICHTUNG	JUNTA
38	900.148.023	1	LID	COUVERCLE	COPERCHIO	DECKEL	TAPA
39	900.102.238	1	SCREW M8x25	VIS M8x25	VITE M8x25	SCHRAUBE M8x25	TORNILLO M8x25
40	900.103.005	10	NUT M 14	ECROU M 14	DADO M 14	MUTTER M 14	TUERCA M 14
41	900.102.027	10	SCREW M 14x35	VIS M 14x35	VITE M 14x35	SCHRAUBE M 14x35	TORNILLO M 14x35
42	900.117.073	1	GUARD	PROTECTION	PROTEZIONE	SCHUTZ	PROTECCION
43	900.102.007	3	SCREW M8x20	VIS M8x20	VITE M8x20	SCHRAUBE M8x20	TORNILLO M8x20
44	900.104.057	3	WASHER 9x24x2	RONDELLE 9x24x2	RONDELLA 9x24x2	ZWISCHENSCHEIBE 9x24x2	ARANDELA 9x24x2
45	900.117.071	1	PROT. HOLDER	DISQUE	FONDELLO	ZWSCHUTZHALTER	DISCO
46	900.102.256	3	SCREW M8x16	VIS M8x16	VITE M8x16	SCHRAUBE M8x16	TORNILLO M8x16

Pag.#

GDT
Rotor

Pag.#

REF	CODE	QTY	ENGLISH	FRANÇAIS	ITALIANO	DEUTSCH	ESPAÑOL	NOTE
1	900.103.105	1	NUT M 36x3	ECROU M 36x3	DADO M 36x3	MUTTER M 36x3	TUERCA M 36x3
2	900.108.007	1	SPLIT PIN 5x50	GOUPILLE 5x50	COPIGLIA 5x50	ARRETIERUNG 5x50	PASADOR 5x50
3	900.112.063	1	PIN	TOURILLON	PERNO	STIFT	PERNO
4	900.112.060	1	GEAR	ENGRENAGE	INGRANAGGIO	ZAHNRAD	ENGRANAJE
5	900.112.079	1	SPACER	ENTRETOISE	DISTANZIALE	ABSTANDSRING	DISTANCIADOR
6	900.103.058	1	RING NUT BLOK M55x2	EMBOUT BLOK M55x2	GHIERA BLOK M55x2	NUTMUTTER BLOK M55x2	CASQUIL. BLOK M55x2
7	900.100.056	2	BEARING 30212	ROULEMENT 30212	CUSCINETTO 30212	KUGELLAGER 30212	COJINETE 30212
8	900.106.034	1	CIRCLIP I 110	SERFLEX I 110	SEEGER I 110	SEEGER I 110	SEEGER I 110
9	900.112.061	1	GEAR	ENGRENAGE	INGRANAGGIO	ZAHNRAD	ENGRANAJE
10	900.103.086	2	RING NUT BLOK M 50x1.5	EMBOUT BLOK M50x1.5	GHIERA BLOK M50x1.5	NUTMUTTER BLOK M50x1.5	CASQUIL. BLOK M50x1.5
12	900.102.027	10	SCREW M 14x35	VIS M 14x35	VITE M 14x35	SCHRAUBE M 14x35	TORNILLO M 14x35
13	900.110.141	1	HUB	MOYEU	MOZZO	NABE	MOZO
14	900.104.114	6	WASHER GROWER 16 R	RONDELLE GROWER 16 R	RONDELLA GROWER 16 R	ZWISCHENSC. GROWER 16 R	ARANDELA GROWER 16 R
15	900.103.063	6	NUT BIBLOK M 16	ECROU BIBLOK M16	DADO BIBLOK M16	MUTTER BIBLOK M16	TUERCA BIBLOK M16
16	900.112.062	1	GEAR	ENGRENAGE	INGRANAGGIO	ZAHNRAD	ENGRANAJE
17	900.106.007	1	CIRCLIP I 120	SERFLEX I 120	SEEGER I 120	SEEGER I 120	SEEGER I 120
18	900.100.089	1	BEARING 22213	ROULEMENT 22213	CUSCINETTO 22213	KUGELLAGER 22213	COJINETE 22213
19	900.101.091	1	WATERPROOF DOUBLE SEAL	DISPOSITIF TENUE	DISPOSITIVO TENUTA	VORRICHTUNG HALTEN	DISPOSITIVO SUJETAR
20	900.102.036	6	SCREW M 16x50	VIS M 16x50	VITE M 16x50	SCHRAUBE M 16x50	TORNILLO M 16x50
21	900.139.010	1	GASKET	JOINT	GUARNIZIONE	DICHTUNG	JUNTA
22	900.111.018	--	BLADE	LAME	ZAPPETTA	MESSER	AZADA
23	900.111.017	--	BLADE	LAME	ZAPPETTA	MESSER	AZADA
24	OPTIONAL	--	BLADE	LAME	ZAPPETTA	MESSER	AZADA
25	OPTIONAL	--	BLADE	LAME	ZAPPETTA	MESSER	AZADA
26	900.102.046	--	SCREW M 14x40x1.5	VIS M 14x40x1.5	VITE M 14x40x1.5	SCHRAUBE M 14x40x1.5	TORNILLO M 14x40x1.5
27	900.110.143	1	SUPPORT	SUPPORT	SUPPORTO	STUETZE	SOPORTE
28	900.103.027	--	NUT BIBLOK M 14x1.5	ECROU BIBLOK M14x1.5	DADO BIBLOK M14x1.5	MUTTER BIBLOK M14x1.5	TUERCA BIBLOK M14x1.5
29	900.107.023	1	RING	ANNEAU	ANELLO	RING	ANILLO
30	900.110.014	1	SUPPORT	SUPPORT	SUPPORTO	STUETZE	SOPORTE
31	900.101.002	2	OIL SEAL 60x80x10	PARE-HUILE 60x80x10	PARAOLIO 60x80x10	SIMMERRING 60x80x10	PARA-ACEITE 60x80X10
32	900.100.018	1	BEARING 6310 2RS	ROULEMENT 6310 2RS	CUSCINETTO 6310 2RS	KUGELLAGER 6310 2RS	COJINETE 6310 2RS
33	900.110.133	1	CLAMPING	CHAPEAU	CAPPELLOTTO	KAPPE	CAPUCHON
34	900.102.056	4	SCREW TCEI M8x14	VIS TCEI M 8x14	VITE TCEU M 8x14	SCHRAUBE TCEI M 8x14	TORNILLO TCEI M 8x14
35	900.110.148	1	ROTOR	ROTOR	ROTORE	ROTOR	ROTOR	230
35	900.110.149	1	ROTOR	ROTOR	ROTORE	ROTOR	ROTOR	250
35	900.110.150	1	ROTOR	ROTOR	ROTORE	ROTOR	ROTOR	280
35	900.110.151	1	ROTOR	ROTOR	ROTORE	ROTOR	ROTOR	300
36	900.103.005	10	NUT M 14	ECROU M 14	DADO M 14	MUTTER M 14	TUERCA M 14
37	900.110.012	1	RING	ANNEAU	ANELLO	RING	ANILLO
38	900.104.061	10	WASHER GROWER 14 R	RONDELLE GROWER 14 R.	RONDELLA GROWER 14 R	ZWISCHENSC. GROWER 14 R	ARANDELA GROWER 14 R
39	900.112.065	1	SPACER	ENTRETOISE	DISTANZIALE	ABSTANDSRING	DISTANCIADOR
40	900.103.102	2	RING NUT M 60x2 KM	EMBOUT M 60x2 KM	GHIERA M 60x2 KM	NUTMUTTER M 60x2 KM	CASQUILLO M 60x2 KM

Pag.#

GDT
Rollers

Pag.#

REF	CODE	QTY	ENGLISH	FRANÇAIS	ITALIANO	DEUTSCH	ESPAÑOL	NOTE
1	900.121.062	1	GUARD	PROTECTION	PROTEZIONE	SCHUTZ	PROTECCION
2	900.102.030	2	SCREW	VIS	VITE	SCHRAUBE	TORNILLO
3	900.103.005	8	NUT	ECROU	DADO	MUTTER	TUERCA
4	900.140.047	2	SUPPORT	SUPPORT	SUPPORTO	STUETZE	SOPORTE
5	900.102.031	6	SCREW	VIS	VITE	SCHRAUBE	TORNILLO
6	900.120.078	2	BUSH	COQUILLE	BOCCOLA	BUCHSE	CASQUILLO
7	900.140.056	2	PLATE	PLAT	PIATTO	PLATTE	PLACA
8	900.104.098	2	WASHER	RONDELLE	RONDELLA	ZWISCHENSCHEIBE	ARANDELA
9	900.140.049.0	1	ARM	BRAS	BRACCIO	ARM	BRAZO
10	900.140.048.0	1	ARM	BRAS	BRACCIO	ARM	BRAZO
11	900.102.235	4	SCREW	VIS	VITE	SCHRAUBE	TORNILLO
12	900.104.043	4	WASHER	RONDELLE	RONDELLA	ZWISCHENSCHEIBE	ARANDELA
13	900.103.023	4	NUT	ECROU	DADO	MUTTER	TUERCA
14	900.140.017	1	BAR	BARRE	BARRA	STANGE	BARRA	230
14	900.140.018	1	BAR	BARRE	BARRA	STANGE	BARRA	250
14	900.140.020	1	BAR	BARRE	BARRA	STANGE	BARRA	280
14	900.140.019	1	BAR	BARRE	BARRA	STANGE	BARRA	300
15	900.102.102	8	SCREW	VIS	VITE	SCHRAUBE	TORNILLO
16	900.104.046	8	WASHER	RONDELLE	RONDELLA	ZWISCHENSCHEIBE	ARANDELA
17	900.103.019	8	NUT	ECROU	DADO	MUTTER	TUERCA
18	900.121.086	2	PLATE	PLAQUE	PIASTRA	PLATTE	PLACA
19	900.102.154	6	SCREW	VIS	VITE	SCHRAUBE	TORNILLO
20	900.104.048	6	WASHER	RONDELLE	RONDELLA	ZWISCHENSCHEIBE	ARANDELA
21	900.103.108	6	NUT	ECROU	DADO	MUTTER	TUERCA
22	900.105.007	4	GREASE NIPPLE	GRAISSEUR	INGRASSATORE	SCHMIERNIPPEL	ENGRASADOR
23	900.121.050	2	ADJUST SCREW	VIS DE REGL.	VITE REGISTRO	EINST.SCHRAUBE	TORNILLO REG
24	900.212.126	2	EXSTENSION	PROLONGE	PROLUNGA	VERLAENGERUNG	PROLONGACION
25	900.140.130	1	PLATE	PLAQUE	PIASTRA	PLATTE	PLACA
26	900.140.128	2	PLATE	PLAQUE	PIASTRA	PLATTE	PLACA
27	900.140.043	1	ROLLER	ROULEAU	RULLO	WALZE	RODILLO	230
27	900.211.043	1	ROLLER	ROULEAU	RULLO	WALZE	RODILLO	250
27	900.140.040	1	ROLLER	ROULEAU	RULLO	WALZE	RODILLO	280
27	900.211.044	1	ROLLER	ROULEAU	RULLO	WALZE	RODILLO	300
28	900.140.011	1	ROLLER	ROULEAU	RULLO	WALZE	RODILLO	230
28	900.211.046	1	ROLLER	ROULEAU	RULLO	WALZE	RODILLO	250
28	900.140.012	1	ROLLER	ROULEAU	RULLO	WALZE	RODILLO	280
28	900.211.047	1	ROLLER	ROULEAU	RULLO	WALZE	RODILLO	300
29	900.140.069	1	ROLLER	ROULEAU	RULLO	WALZE	RODILLO	230
29	900.211.052	1	ROLLER	ROULEAU	RULLO	WALZE	RODILLO	250
29	900.140.071	1	ROLLER	ROULEAU	RULLO	WALZE	RODILLO	280
29	900.211.053	1	ROLLER	ROULEAU	RULLO	WALZE	RODILLO	300
30	900.116.035	-	U-BOLT	MANILLE	CAVALLOTTO	U-BOLZEN	SOPORTE
31	900.211.057.0	-	SCRAPER	RACLEUR	RASCHIARULLO	WALZENSCHABER	RASCARODILLO
32	900.104.046	-	WASHER	RONDELLE	RONDELLA	ZWISCHENSCHEIBE	ARANDELA
33	900.103.019	-	NUT	ECROU	DADO	MUTTER	TUERCA
34	900.140.081	1	BAR	BARRE	BARRA	STANGE	BARRA	230
34	900.140.082	1	BAR	BARRE	BARRA	STANGE	BARRA	250
34	900.140.083	1	BAR	BARRE	BARRA	STANGE	BARRA	280
34	900.140.084	1	BAR	BARRE	BARRA	STANGE	BARRA	300
35	900.210.086	-	SCRAPER	RACLEUR	RASCHIARULLO	WALZENSCHABER	RASCARODILLO
36	900.100.051	2	SUPPORT	SUPPORT	SUPPORTO	STUETZE	SOPORTE
37	900.103.069	2	RING NUT	EMBOUT	GHIERA	NUTMUTTER	CASQUILLO
38	900.107.024	-	SHIM	EPAISSEUR REG.	SPESSORE REG.	STAERKE	ESPESOR REG.
39	900.102.115	8	SCREW	VIS	VITE	SCHRAUBE	TORNILLO
40	900.103.019	12	NUT	ECROU	DADO	MUTTER	TUERCA
41	900.104.046	4	WASHER	RONDELLE	RONDELLA	ZWISCHENSCHEIBE	ARANDELA
42	900.102.288	4	SCREW	VIS	VITE	SCHRAUBE	TORNILLO
43	900.102.194	10	SCREW	VIS	VITE	SCHRAUBE	TORNILLO
44	900.104.046	10	WASHER	RONDELLE	RONDELLA	ZWISCHENSCHEIBE	ARANDELA
45	900.103.019	10	NUT	ECROU	DADO	MUTTER	TUERCA
46	900.116.115	2	U-BOLT	MANILLE	CAVALLOTTO	U-BOLZEN	SOPORTE
47	900.140.131	2			FISSAGGIO VITE
48	900.102.387	2	SCREW	VIS	VITE	SCHRAUBE	TORNILLO
49	900.104.046	4	WASHER	RONDELLE	RONDELLA	ZWISCHENSCHEIBE	ARANDELA
50	900.103.019	4	NUT	ECROU	DADO	MUTTER	TUERCA
51	900.104.048	2	WASHER	RONDELLE	RONDELLA	ZWISCHENSCHEIBE	ARANDELA
52	900.103.106	2	NUT	ECROU	DADO	MUTTER	TUERCA
53	900.114.141	2	SHIELD	CAPOT	COFANO	HAUBE	CARCASA	230
53	900.114.142	2	SHIELD	CAPOT	COFANO	HAUBE	CARCASA	250
53	900.114.143	2	SHIELD	CAPOT	COFANO	HAUBE	CARCASA	280
53	900.114.144	2	SHIELD	CAPOT	COFANO	HAUBE	CARCASA	300
54	900.140.129	1	PLATE	PLAQUE	PIASTRA	PLATTE	PLACA
55	900.211.028	2	BUSH	COQUILLE	BOCCOLA	BUCHSE	CASQUILLO
56	900.104.043	2	WASHER	RONDELLE	RONDELLA	ZWISCHENSCHEIBE	ARANDELA
57	900.103.023	2	NUT	ECROU	DADO	MUTTER	TUERCA
58	900.114.097	1	FLAP SHIELD	AILETTE ROUL.	ALETTA RULLO	WALZENHAUBE	ALETA RODIL.
59	900.114.096	1	FLAP SHIELD	AILETTE ROUL.	ALETTA RULLO	WALZENHAUBE	ALETA RODIL.

Pag.#

GDT
Rollers

Pag.#

REF	CODE	QTY	ENGLISH	FRANÇAIS	ITALIANO	DEUTSCH	ESPAÑOL	NOTE
60	900.102.098	6	SCREW	VIS	VITE	SCHRAUBE	TORNILLO
61	900.103.019	6	NUT	ECROU	DADO	MUTTER	TUERCA
62	900.114.145	6	FLASK	MOULE	STAFFA	KLAUE	PLETINA
63	900.102.100	16	SCREW	VIS	VITE	SCHRAUBE	TORNILLO
64	900.104.045	16	WASHER	RONDELLE	RONDELLA	ZWISCHENSCHEIBE	ARANDELA
65	900.103.018	16	NUT	ECROU	DADO	MUTTER	TUERCA
66	900.275.018	1	CYLINDER	VERIN	CILINDRO	ZYLINDER	CILINDRO
67	900.102.290	1	SCREW	VIS	VITE	SCHRAUBE	TORNILLO
68	900.104.072	1	WASHER	RONDELLE	RONDELLA	ZWISCHENSCHEIBE	ARANDELA
69	900.103.108	1	NUT	ECROU	DADO	MUTTER	TUERCA
70	900.102.380	1	SCREW	VIS	VITE	SCHRAUBE	TORNILLO
71	900.104.048	1	WASHER	RONDELLE	RONDELLA	ZWISCHENSCHEIBE	ARANDELA
72	900.103.106	1	NUT	ECROU	DADO	MUTTER	TUERCA
73	900.104.039	4	WASHER	RONDELLE	RONDELLA	ZWISCHENSCHEIBE	ARANDELA
74	900.102.269	2	BOLT DRILLED	BOULON AVEC TROUS	BULLONE FORATO	SCHRAUBB. GEBORTH	BULON OJOS
75	900.276.020	2	PIPE	TUBE	TUBO	ROHR	TUBO
76	900.237.156	2	NIPPLES	NIPPLES	NIPPLES	NIPPEL	NIPPLES
77	900.104.033	2	WASHER	RONDELLE	RONDELLA	ZWISCHENSCHEIBE	ARANDELA
78	900.237.174	2	JACK	EMBRAYAGE	INNESTO	VERBINDEN	CONEXION

Pag.#

LIMITED WARRANTY POLICY
SOVEMA Srl, Manufacturer of quality machinery, guarantees new Sovema machinery from the time of delivery to the original purchaser to be free from defects in material and workmanship if properly set up and operated in accordance with recommendations set forth in SOVEMA’s operator manual. SOVEMA’s liability for any defect of accepted goods shall be limited to replacing them, or as SOVEMA shall elect.
The original purchaser will qualify for the SOVEMA warranty only after they have completed the warranty card in full and forwarded it to SOVEMA Srl Italy or any SOVEMA branch.
SOVEMA’s obligation shall terminate 12 (twelve) months after the date of purchase of the product by the original purchaser. This warranty cannot be assigned or transferred to anyone unless SOVEMA’s consent in writing has first been obtained. All warranty claims must be forwarded to SOVEMA Srl Italy or a SOVEMA branch within 8 (eight) days after occurrence.
The original purchaser will be responsible for and bear costs of:
Normal maintenance such as greasing, maintenance of oil levels, minor adjustments, etc.
Transportation of any kind of, any SOVEMA product to and from the place where warranty work is performed.
This warranty shall not apply to any machine which has been repaired or altered in any way outside the SOVEMA factory which affects its stability or reliability, nor which has been subject to misuse, negligence or accident, nor to any machine that has not been operated in accordance with SOVEMA’s printed instructions, or operated beyond the company recommended capacity as per machine.
This warranty shall not be applicable to items which are subject to the warranties of their respective manufacturers. Such items would include but would not be limited to clutches, universal joints, knives, hydraulic components, bearings, tires, belts and other trade accessories.
This warranty shall not be applicable to items defined as normal wearing items. Such items would include but would not be limited to belts, discs, knives, tines stone guards, tires, slip clutches, pitman shaft, swath sticks, blades or tine holders.
The judgement of SOVEMA Srl in all cases of claims under this warranty shall be final and conclusive and the original purchaser agrees to accept its decisions about all questions as to defects and/or to the exchange of any part or parts.
No Agent, Employee or Representative of SOVEMA has any authority to bind SOVEMA to any affirmation, representation or warranty, concerning its machinery excepts as specifically set forth.
SOVEMA shall not be liable for special or consequential damages of any kind caused by any SOVEMA product.

Pag.#

SOVEMA Srl
Via Olmo, 6-8-10
41013 Gaggio di Piano (MO)
Italy

Pag.#

Pag.#

SOVEMA Srl
Via Olmo, 6-8-10
41013 Gaggio di Piano (MO)
Italy

Pag.#

SOVEMA Product Line
SIDE SHIFT ROTARY TILLERS
15 different models;
For tractors from 12 to 70 HP
Working width from 80 to 200 cm.
FIXED ROTARY TILLERS
Over 45 different models;
For tractors from 15 to 130 HP
Working width from 80 to 300 cm.
STONE BURRIERS
6 different models;
For tractors from 35 to 90 HP
Working width from 100 to 200 cm.
ROTARY HARROWS
13 different models;
For tractors from 25 to 150 HP
Working width from 110 to 500 cm.
ROTARY DITCHERS
10 different models;
For tractors from 40 to 130 HP
Working depth from 45 to 110 cm.

Pag.#

FLAIL MOWERS - SHREDDERS
35 different models;
For tractors from 15 to 120 HP
Working width from 100 to 470 cm.
MOWERS COLLECTOR
6 different models;
For tractors from 30 to 60 HP
Working width from 120 to 180 cm.
Available with high discharge and low discharge
FINISHING MOWERS
14 different models;
For tractors from 15 to 70 HP
Working width from 100 to 300 cm.
HYDRAULIC FORK-LIFTS
11 different models;
For tractors up to 60 HP
Lifting capacity from 1.300 Kg to 2.000 Kg.
TRACTOR CABS
Over twenty models of cabs for eleven manufacturers of tractors;
For tractors with wheels or crawlers;
All models available with heating and/or air conditioned.

Pag.#

ROTARY RAKE
4 different models
For tractors from 30 to 70 HP
Working width from 340 to 695 cm.
HAY TEDDERS
6 different models (2, 4, 6 rotors)
For tractors from 10 to 40 HP
Working width from 310 to 730 cm.
SICKLE BAR MOWER
3 different models.
For tractors from 10 to 15 HP.
FINGER WHEELS
8 different models (8-20 stars)
For tractors from 30 to 80 HP
Working width from 7.35 to 12.50 m.

Pag.#